set interfaces ethernet eth0 address '10.0.17.151/24'
set interfaces ethernet eth0 description 'SEC350-WAN'
set interfaces ethernet eth1 address '172.16.50.2/29'
set interfaces ethernet eth1 description 'CHARLOTTE-DMZ'
set interfaces ethernet eth2 address '172.16.150.2/24'
set interfaces ethernet eth2 description 'CHARLOTTE-LAN'
set nat source rule 10 description 'NAT FROM DMZ to WAN'
set nat source rule 10 outbound-interface 'eth0'
set nat source rule 10 source address '172.16.50.0/29'
set nat source rule 10 translation address 'masquerade'
set nat source rule 20 description 'NAT from LAN to WAN'
set nat source rule 20 outbound-interface 'eth0'
set nat source rule 20 source address '172.16.150.0/24'
set nat source rule 20 translation address 'masquerade'
set nat source rule 30 description 'NAT from MGMT to LAN'
set nat source rule 30 outbound-interface 'eth0'
set nat source rule 30 source address '172.16.200.0/28'
set nat source rule 30 translation address 'masquerade'
set protocols rip interface eth2
set protocols rip network '172.16.50.0/29'
set protocols static route 0.0.0.0/0 next-hop 10.0.17.2
set service dns forwarding allow-from '172.16.50.0/29'
set service dns forwarding allow-from '172.16.150.0/24'
set service dns forwarding listen-address '172.16.50.2'
set service dns forwarding listen-address '172.16.150.2'
set service dns forwarding system
set service ssh listen-address '0.0.0.0'
set system host-name 'fw01-charlotte'
set system name-server '10.0.17.2'
